Warning

Proper installation and consistent use of the 5 point harness restraint system is critical to your safety in event of accident. To reduce risk of serious injury or death:

Follow vehicle manufacturers, and PRP Seats instructions and safety messages during installation and use of this product.

Use all belts provided. Secure lap belt first; low and snug across hips. Sternum strap tight at chest line (min. 4” below neck). Adjust remaining straps per instructions and confirm fitment restrains user & provides safe clearance from wheel, dash, roll cage, etc.

Inspect all components of the 5 point harness restraint system regularly & replace as indicated by accident, wear or abrasion. Replace no later than 2 years from date on SFI 16.1 tag.

This 5 point competition restraint system is intended for UTV or other off-road vehicle-not replacement for FMVSS 209 restraints. Never use with child car seats or boosters.